Quiz on SQR function

What is the job of register bl?

What is the job of register cl?

Register cl gets the value zero 2 times. Why?

What does the instruction Ret do?

What are the 3 options for the instruction Cmp al,0?

Which register holds the result when it returns to the main program?